**MikroTik LAN Hotspot**

**Step1:**

*bridge > bridge name > click apply and ok*

**Step2:**

*bridge > ports > + > add LAN interface > select bridge > click apply and ok*

**Step3:**

*IP > DHCP client > add client (WAN) > click apply and ok*

**Step4:**

*IP > address > add bridge static IP > click apply and ok*

**Step5:**

*IP > Hotspot > server > hotspot setup > select bridge interface > add DNS , DNS name > done*

**:::MAKE user:::**

*IP > Hotspot > user > username, password > click apply and ok*